# TT-S6/D updates and changes

In this document you find what has been updated between the different releases for TT-S6/D

## Version 2 - Rev 1 – 24-12-20

* Modified function so that when the input goes below 0.5V, all outputs are turned off disregarding the step delay.